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BRAND FORMING MACHINERY CO.,LIMITED
VENTILATION FRAME ROLL FORMING MACHINE
◎PROFILE(AUTO Change Size By Motor Drive,One Minute Finish)
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
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◎Material Information
Applicable Material:Galvanized Steel       Material Thickness:0.5-0.7mm
The Width Of Tolerance:±0.5mm
The Height Of Tolerance:±0.5mm
The Length Of Tolerance:±1mm
◎Work Flow(Machine Space:18000*2500mm)
Manual Uncoiler→Feeding Guide Device→Leveling Device→Hydraulic Pre Punching Hole Device→Main Forming Mill→Straighter Device→Hydraulic AUTO Cutting & Bending Device→Exit Rack
www.rollforming-machinery.com
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
◎Manual Uncoiler:One Set
Manual Control Steel Coil Inner Bore Shrinkage And Stop
Max. Feeding Width:300mm,Coil ID Range:508+/-30mm
Max Capacity:2 T
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◎Feeding Guide Device:One Set
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
◎Leveling Device:One Set
Up Three Down Four Totally Seven Shafts Leveling Device
With Feeding Material Guide, Body Frame Made From H450 Type Steel By Welding Side Wall Thickness: Q235 t18mm;Tie rod:ф22 Galvanized
Shafts Make From 45# Steel,Diameter=φ90mm,High Frequency Heat Treatment
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◎Hydraulic Punching Device
Pre-Punching & Post Cutting & Bending,Use The Same Hydraulic System Hydraulic Motor:7.5KW,Hydraulic Pressure Range:0-16Mpa
Punching Tool Material:Cr12MoV(=D2 Steel),Heat Treatment To HRC58-62 6-Hydraulic Cylinders Punching System For Punching
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
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A Cylinder：①+② - Four sets of molds
B Cylinder：⑥ - Four sets of molds
C Cylinder：③ - Four sets of molds
D Cylinder：④ - One set of mold
E Cylinder：⑦ - One set of mold
F Cylinder：⑤ - One set of mold
www.rollforming-machinery.com
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
◎Main Forming Mill
Body Frame Made From H450 Type Steel By Welding
Archway Structure For More Stable
Profile Size Change By Motor Drive
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Main Servo Motor=7.5KW, Frequency Speed Control
Speed Reducer Motor:K Series
Gear Box Driving,14-Steps To Form Profile
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
Real Forming Speed:20m/min
Rollers Make From GCr15 Steel,Heat Treatment,HRC 58-62 Degree Shafts Diameter=ф65,Quenching And Tempering
All The Screw Bolts With Grade 8.8
◎Post Hydraulic AUTO Cutting & Bending Device:One Set
Post To Cut, Stop To Cutting,Two Pieces Type Of Cutting Blade Design Hydraulic Motor:7.5KW;Cutting pressure: 0-16Mpa
Cutting Tool Material:Cr12MoV(= SKD11 With At Least One Million Times Of Cutting Life),Heat Treatment To HRC58-62 Degree
The Cutting Power Is Provided By The Main Engine Hydraulic Station
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
◎PLC Control System:One Set
Control The Quantity And Cutting Length Automatically Input The Production Data(Production,Batch,Piece,Length,etc.)On The Touch Screen,It Can Finish The Production Automatically.Combined With: PLC, Inverter, Touch Screen, Encoder Switch Bottom, Indicate Light, Power Supply, Intermediate Relay, AC Contactor PLC:Siemens(German Brand);
Inverter:SHILIN(Taiwan Brand)
7-Inch Color Touch Screen:Siemens(German Brand)
Encoder:Omron (Japan Brand);Thermal Relay:Schneider(France Brand) Air Switch:LG-LS(Korea Brand);Cut-to-Length Tolerance≤±1 mm Control Voltage 24V
Chinese And English Language
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
◎Exit Rack:3m Length One Set

◎Tools And Spare Parts:One Set
Open Wrench 24x22, 22x19, 19x17, 17x14 A Hex Wrench (Size 1 to 10)
A Vise,A Cross And A Flat-Head Screwdriver, A Feeler,A Iron A Hammer, A Tape Measure
Spare Parts: 1.Drive Chain x 1
2.Drive Bearing x 2 3.Limited Switch x 1
www.rollforming-machinery.com
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BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
◎ Sample Show


www.rollforming-machinery.com
- 12
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Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
◎Machine Show


www.rollforming-machinery.com
- 13
BRAND FORMING MACHINERY CO.,LIMITED
Tel/Whatsapp:0086-13395014880
E-mail:sales03@rollformerschina.com
VENTILATION FRAME ROLL FORMING MACHINE
◎Price
	NO.
	Item Name
	Quality
	Delivery Time
	

	
	
	
	
	

	1
	Manual Uncoiler
	1
	
	

	
	
	
	
	

	2
	Feeding Guide Device
	1
	
	

	
	
	
	
	

	3
	Leveling Device
	1
	
	

	
	
	
	
	

	4
	Punching Hole device
	1
	
	

	
	
	
	
	

	5
	Punching Mold
	15
	
	

	
	
	
	
	

	6
	Roll Forming Mill
	1
	75 Workdays
	

	
	
	
	
	

	7
	Hydraulic Post AUTO Cutting &
	1
	
	

	
	
	
	
	

	
	Bending Device
	
	
	

	
	
	
	
	

	8
	Cutting Mold
	4
	
	

	
	
	
	
	

	9
	Hydraulic Station
	1
	
	

	
	
	
	
	

	10
	PLC Control System
	1
	
	

	
	
	
	
	

	11
	Exit Rack
	1
	
	

	
	
	
	
	

	12
	Tools And Spare Parts
	1
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